Run start : 2018-06-17 2133
Input file name : 7f0105a0945579797df268c079af6110

Domain settings:
Latitude of domain centre =  50.612732
Longitude of domain centre = **********
Latitude of domain lower left =  50.576279
Longitude of domain lower left = **********
Latitude of domain upper left =  50.649123
Longitude of domain upper left = **********
Latitude of domain lower right =  50.576279
Longitude of domain lower right = **********
Latitude of domain upper right =  50.649123
Longitude of domain upper right = **********
nTiles = 1080
nXtiles = 40
nYtiles = 27
nXpertile = 10
nYpertile = 10
nXPoints = 400
nYPoints = 270
Xtilesize =  300.00
Ytilesize =  300.00
xSize =  12000.00
ySize =   8100.00
deltaX =  30.000
deltaY =  30.000

Initial Conditions:
Number of cap sources = 1
Cap 1 :
x position = -3984.560858
y position =  1143.286605
latitude =    50.623000
longitude =  -123.503000
radius =   600.000000
volume = 6.105080E+07
height =    53.980759
concentration =     0.600000
shape = flat

Parameters:
g =  9.81
rhow =  1000.00
rhos =  2000.00
reduced g =  9.81
Drag : Voellmy+Pouliquen
Chezy coefficient =  0.02
Pouliquen Min Slope =  0.20
Pouliquen Max Slope =  0.50
Voellmy switch rate =  3.00
Voellmy switch value =  0.20
Erosion : On
Erosion rate =  1.00E-03
Critical shields =  0.06
Erosion depth =  1.00
Erosion critical height =  0.01
Bed porosity =  0.35
Maximum packing fraction =  0.65
Solid diameter = 1.000E-02
Particle Reynolds number = 2.610E+03
Particle settling speed in clear water = 3.194E-01
Exponent in hindered settling term = 2.379E+00

Solver settings:
limiter : MinMod2
precusor layer depth =  0.00E+00
height threshold =  1.00E-08
tile buffer = 3
cfl number =  0.25
max time step = 10.00
end time =  1000.00

Output settings:
Number of output files = 100
Time step between outputs =   10.00
Last output file = 100

Topographic settings:
Topography type = SRTM1
Topography path = /srv/projects/lahars/var/www/LaharFlow/records/dem/7f0105a0945579797df268c079af6110/
